## SH-500HD REPAIR INSTRUCTIONS

Use this repair on SH-500HD that has a blank screen or can not start the MENU.
(DO NOT CHANGE THE FILE NAME)

1. IMPORTANT: Format your USB flash drive to FAT or FAT32
2. Copy the repair software (V5_fix.rcv) to the USB flash drive root directory
   Note: DO NOT CHANGE FILE NAME
3. Insert USB flash drive into the meters USB interface
4. Press and hold F1 and turn on your meter
5. Release the F1 button when all LED lights
6. Wait 5 minutes
7. Turn off your meter
8. Remove the USB flash drive
9. Restart your meter

Software Notice

All software is offered "as is" and without guarantee. This software is for experienced users only. If you don't have the ability to load this software or if you feel unsure of your abilities, DO NOT use this software. DMS International is in no way responsible for the use or mis-use of this software. Any repairs required because of your use or mis-use of this software will be charged at normal bench repair rates and normal replacement parts cost. By using this software you are agreeing to these terms.

USE THIS SOFTWARE AT YOUR OWN RISK

These files may NOT be freely distributed and may NOT modified in any way. This comment must remained attached to the files.

Quick Links

- DMS International - Email Sales
- First Strike Meters - Email Sales
- Sathero Meters - Email Sales
- Trimax Meters - Email Sales
- 8dtek Meters - Email Sales